{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["COrE+ light","COrE+ Extended","Feuil1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":6,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1904","formulas":"cached_only"}

{"sheet":"COrE+ light","index":0,"n_rows":131,"n_cols":30,"rows_kept":131,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["COrE+ LIGHT sensitivity estimate","V0.91"]
["M. Piat, J. Delabrouille"]
["2014-10-28"]
[{"$nulls":17},"Core channels"]
["nu (GHz)","[GHz]","nu",null,null,null,60,70,80,90,100,115,130,145,160,175,195,220,255,295,340,390,450,520,600,700,800,950,1100,1250]
["Number of detectors (2 x nb of horns)",{"$nulls":5},10,10,20,30,50,100,160,240,260,300,350,200,120,60,40,30,20,20,20,0,0,0,0,0]
["Scaling factor",null,null,null,1]
["Total number of detectors",null,null,null,2040]
[]
["Parameter","Units","Formula","Values"]
[]
["Mission duration","[yr]","tmiss",3]
[]
["Rotation speed","[rpm]","w",2]
["Boresight angle","[°]","b",45]
["Scanning speed","[°/s]","ss=2pi*sin(b)/60*w",8.48528137423857]
[]
["Telescope diameter","m","Dtel",1]
["Telescope f number",null,"f#=F/D",2]
["Telescope temperature","[K]","Ttel",40]
["Telescope emissivity","[%]","e_tel",0.5]
["Payload enclosure temperature","[K]",null,40]
[]
["Lambda center","[mm]","la",null,null,null,5,4.285714285714286,3.75,3.3333333333333335,3,2.608695652173913,2.3076923076923075,2.0689655172413794,1.875,1.7142857142857142,1.5384615384615385,1.3636363636363635,1.1764705882352942,1.0169491525423728,0.8823529411764706,0.7692307692307693,0.6666666666666666,0.5769230769230769,0.5,0.42857142857142855,0.375,0.3157894736842105,0.2727272727272727,0.24]
["dnu/nu",{"$nulls":5},0.35,0.35,0.25,0.35,0.2,0.1,0.28,0.35,0.28,0.35,0.2,0.35,0.12,0.2,0.35,0.2,0.35,0.2,0.35,0.35,0.35,0.35,1.35,0.35]
["dnu","[GHz]","dnu",null,null,null,21,24.5,20,31.499999999999996,20,11.5,36.400000000000006,50.75,44.800000000000004,61.24999999999999,39,77,30.599999999999998,59,118.99999999999999,78,157.5,104,210,244.99999999999997,280,332.5,1485,437.5]
["Beam étendue","[m^2.sr]","Aomega=la^2",null,null,null,2.5e-05,1.836734693877551e-05,1.40625e-05,1.1111111111111113e-05,9e-06,6.805293005671079e-06,5.3254437869822475e-06,4.2806183115338884e-06,3.515625e-06,2.938775510204081e-06,2.3668639053254444e-06,1.8595041322314046e-06,1.3840830449826992e-06,1.0341855788566503e-06,7.785467128027683e-07,5.917159763313611e-07,4.4444444444444444e-07,3.3284023668639047e-07,2.5e-07,1.8367346938775507e-07,1.40625e-07,9.97229916897507e-08,7.43801652892562e-08,5.76e-08]
["Airy disk diameter (first zeros)","[arcmin]","1,22*la/Dtel",null,null,null,20.97025530178813,17.974504544389827,15.7276914763411,13.980170201192086,12.58215318107288,10.941002766150328,9.67857937005606,8.677347021429572,7.86384573817055,7.18980181775593,6.45238624670404,5.719160536851309,4.9341777180677955,4.2651366715501275,3.7006332885508466,3.22619312335202,2.7960340402384167,2.419644842514015,2.0970255301788128,1.7974504544389824,1.57276914763411,1.3244371769550396,1.1438321073702618,1.0065722544858302]
["Edge taper","dB","EdB",null,null,null,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23]
["Spill over (assuming gaussian beam)","%",{"$nulls":4},0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721]
["Pure gaussian beam FWHM","[arcmin]","FWHM=2.355*la/(2*pi*Dtel/(sqrt(-2*EdB/10*ln(10)))",null,null,null,20.96726047428804,17.971937549389747,15.725445355716033,13.978173649525361,12.580356284572822,10.93944024745463,9.677197141979095,8.676107782464015,7.862722677858017,7.188775019755897,6.451464761319397,5.71834376571492,4.933473052773658,4.264527554092482,3.7001047895802417,3.2257323806596987,2.7956347299050712,2.4192992854947737,2.0967260474288043,1.7971937549389743,1.5725445355716028,1.324248029955034,1.143668753142984,1.0064285027658257]
["Beam FWHM (Goldsmith)","[arcmin]","FWHM=(1.02-0.0135*EdB)*la/Dtel",null,null,null,22.869610392646813,19.60252319369727,17.152207794485104,15.246406928431208,13.721766235588087,11.931970639641815,10.555204796606219,9.463287059026266,8.576103897242552,7.841009277478904,7.03680319773748,6.237166470721856,5.381084798269839,4.651446181555283,4.0358135987023775,3.51840159886874,3.0492813856862413,2.6388011991515548,2.2869610392646806,1.960252319369726,1.7152207794485108,1.4443964458513772,1.2474332941443713,1.0977412988470467]
[null,"[arcsec]","FWHM",{"$nulls":20},158.32807194909327,137.21766235588083,117.61513916218357,102.91324676691065,86.66378675108263,74.84599764866228,65.8644779308228]
["Polarisation efficiency",null,"eta_pol",null,null,null,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,2,1]
[]
["Bolometer performances"]
["Detection efficiency","[%]","eff",null,null,null,50,50,50,50,50,50,50,50,50,50,50,50,50,50,50,50,50,50,50,50,50,50,50,50]
["Power per mode","[W]","Pmode=eff*e_tel*bnu*Aomega*dnu/2",null,null,null,2.7892389032181035e-13,2.9922683448777037e-13,2.245687675544732e-13,3.251966058560068e-13,1.899037203851935e-13,9.644169680064372e-14,2.7026939369821647e-13,3.347865305058596e-13,2.637451799394302e-13,3.235368806765153e-13,1.8002096453530662e-13,3.0562006179904314e-13,1.0181641832965926e-13,1.6838386023880023e-13,3.006625620182054e-13,1.7989261806570944e-13,3.3742526617831547e-13,2.0930264926166978e-13,3.9813517887979943e-13,4.3315845764427337e-13,4.61881167781848e-13,4.935368034593584e-13,1.9785748184504547e-12,5.219496982919094e-13]
["Shot noise","[W/sqrt(Hz)]",{"$nulls":4},4.707198088795989e-18,5.266150683404963e-18,4.877122497884363e-18,6.2249841408474104e-18,5.014304795183438e-18,3.831998532732759e-18,6.820466849368672e-18,8.017001816546815e-18,7.47474273258745e-18,8.658146178758396e-18,6.817463797023456e-18,9.435094678953958e-18,5.8630418006747624e-18,8.109708264300918e-18,1.1633841107652938e-17,9.637912235770241e-18,1.417878604073848e-17,1.2004194598709003e-17,1.7784222954689716e-17,2.0036248614566365e-17,2.211842066953546e-17,2.4915268238395123e-17,5.3680502657773635e-17,2.939092973475167e-17]
["Photon NEP","[W/sqrt(Hz)]","NEPphot",null,null,null,5.437563634985991e-18,5.9195828622795395e-18,5.369305075655816e-18,6.7427659833954344e-18,5.36186486967113e-18,4.037546052444682e-18,7.108604612453434e-18,8.287903449302738e-18,7.679661705814103e-18,8.853332185365847e-18,6.9382806332244796e-18,9.562796646862371e-18,5.920541664714059e-18,8.168750883256995e-18,1.1698955194193688e-17,9.680864143917503e-18,1.4229678902061597e-17,1.2039233438652389e-17,1.7826615511212568e-17,2.0074434024330357e-17,2.2152840646805515e-17,2.4944653248444426e-17,5.372958930941612e-17,2.94121089308305e-17]
["Bolometer NEP","[W/sqrt(Hz)]","NEPphot",null,null,null,5.437563634985991e-18,5.9195828622795395e-18,5.369305075655816e-18,6.7427659833954344e-18,5.36186486967113e-18,4.037546052444682e-18,7.108604612453434e-18,8.287903449302738e-18,7.679661705814103e-18,8.853332185365847e-18,6.9382806332244796e-18,9.562796646862371e-18,5.920541664714059e-18,8.168750883256995e-18,1.1698955194193688e-17,9.680864143917503e-18,1.4229678902061597e-17,1.2039233438652389e-17,1.7826615511212568e-17,2.0074434024330357e-17,2.2152840646805515e-17,2.4944653248444426e-17,5.372958930941612e-17,2.94121089308305e-17]
["Total NEP","[W/sqrt(Hz)]",{"$nulls":4},7.689876238863935e-18,8.371554367427071e-18,7.593344058511152e-18,9.535711101625783e-18,7.582822018300759e-18,5.709952386073221e-18,1.0053085052479585e-17,1.1720865461642687e-17,1.0860681738799602e-17,1.2520502448738614e-17,9.812210571056646e-18,1.3523836712208722e-17,8.372910318833605e-18,1.1552358286749242e-17,1.654482110122388e-17,1.3690809367819535e-17,2.0123804891509802e-17,1.702604720951788e-17,2.5210641427167398e-17,2.8389536854171904e-17,3.132884768780233e-17,3.527706693264419e-17,7.598511390211274e-17,4.1595003347975325e-17]
["NET per bolo","[μKCMB.sqrt(s)]",{"$nulls":4},41.07157907910982,39.60532533860055,45.69527933374297,38.0104014256849,49.89302043013546,70.68887039347355,42.94881558573445,39.58865075769985,46.202793410485675,43.67006061523924,63.330656371454,55.22683625141123,120.92334763823648,132.25665093497176,157.0778446396144,364.5341740083578,573.9608514304623,1889.6761491857726,4257.127912731676,17557.34725103984,75485.22121912311,711859.1749355365,3591216.287961648,72469004.5765045]
[]
["Beam duration","[ms]","∆t_beam=FWHM/ss",null,null,null,44.92015719926362,38.502991885083105,33.690117899447706,29.946771466175747,26.95209431955817,23.436603756137544,20.732380245813975,18.587651254867705,16.845058949723853,15.401196754033236,13.82158683054265,12.250951963435531,10.569448752767913,9.13630315917226,7.927086564575931,6.910793415271325,5.98935429323515,5.183095061453494,4.4920157199263615,3.850299188508309,3.3690117899447714,2.837062559953491,2.450190392687106,2.1561675455646534]
["Required time constant","[ms]","tau=tbeam/(3pi)",null,null,null,4.7661767084851965,4.08529432155874,3.5746325313638962,3.177451138990131,2.8597060250911177,2.486700891383581,2.1997738654547057,1.9722110517869778,1.7873162656819481,1.6341177286234954,1.466515910303137,1.299866375041417,1.1214533431729876,0.969391872912243,0.8410900073797403,0.7332579551515686,0.6354902277980262,0.5499434663636764,0.4766176708485196,0.40852943215587384,0.3574632531363897,0.3010216868516965,0.2599732750082834,0.22877648200728937]
[null,"[µs]","tau",null,null,null,4766.176708485196,4085.2943215587397,3574.6325313638963,3177.451138990131,2859.7060250911177,2486.700891383581,2199.7738654547056,1972.2110517869778,1787.3162656819482,1634.1177286234954,1466.5159103031372,1299.866375041417,1121.4533431729876,969.391872912243,841.0900073797403,733.2579551515686,635.4902277980262,549.9434663636764,476.6176708485196,408.52943215587385,357.4632531363897,301.02168685169653,259.9732750082834,228.77648200728936]
[]
["Sampling"]
["Number of sample per beam",null,"Nsbeam",null,null,null,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["Sampling frequency","[Hz]","fsamp",null,null,null,89.04688339037185,103.88803062210049,118.72917785382917,133.57032508555778,148.4114723172864,170.67319316487936,192.93491401247238,215.1966348600653,237.45835570765834,259.7200765552513,289.4023710187086,326.50523909803013,378.44925440908025,437.81384333599505,504.59900587877394,578.8047420374172,667.8516254277889,771.7396560498895,890.4688339037185,1038.8803062210052,1187.2917785382913,1409.908987014221,1632.526195490151,1855.1434039660803]
["Coding in bits per bolometer","[bits]","Nbits",null,null,null,16,16,16,16,16,16,16,16,16,16,16,16,16,16,16,16,16,16,16,17,18,19,20,20]
["Data rate per bolometer","[kbits/s]","fsamp*Nbits/1000",null,null,null,1.4247501342459494,1.6622084899536078,1.8996668456612666,2.1371252013689244,2.3745835570765825,2.7307710906380698,3.086958624199558,3.4431461577610447,3.7993336913225333,4.155521224884021,4.630437936299337,5.224083825568482,6.055188070545284,7.005021493375921,8.073584094060383,9.260875872598675,10.685626006844622,12.347834496798232,14.247501342459497,17.66096520575709,21.37125201368924,26.7882707532702,32.65052390980302,37.1028680793216]
["Data rate per channel","[kbits/s]",{"$nulls":4},14.247501342459493,16.622084899536077,37.993336913225335,64.11375604106773,118.72917785382913,273.077109063807,493.91337987192924,826.3550778626508,987.8267597438587,1246.6563674652064,1620.653277704768,1044.8167651136964,726.622568465434,420.30128960255524,322.9433637624153,277.82627617796027,213.71252013689244,246.95668993596462,284.95002684918995,0,0,0,0,0]
[]
["Total data rate","[kbits/s]",{"$nulls":4},9238.317328806446]
["Compression factor",{"$nulls":5},4]
["Total data rate with compresion","[kbits/s]",{"$nulls":4},2309.5793322016116]
[]
["Sensitivity per horn"]
["Number of pixel of diam FWHM",null,"Npix",null,null,null,361534.8907296098,492089.15682641335,642728.6946304179,813453.5041416222,1004263.5853600275,1328138.591638636,1697205.459258447,2111464.188219458,2570914.7785216714,3075557.230165086,3818712.283331505,4860635.753142535,6530223.963803576,8739603.851595642,11609287.046761924,15274849.13332602,20336337.60354056,27155287.34813515,36153489.072960995,49208915.68264138,64272869.46304176,90634788.57874252,121515893.82856338,156916185.21250436]
["int time per pixel of diam FWHM","[s]","tint",null,null,null,261.86352251906254,192.389526748699,147.29823141697258,116.38378778625001,94.2708681068625,71.28231992957468,55.781578761457084,44.837511584714626,36.824557854243146,30.782324279791816,24.79181278286982,19.477452088194724,14.49763446472319,10.832619144712723,8.154919386406785,6.197953195717455,4.655351511449999,3.4863486725910677,2.6186352251906246,1.9238952674869885,1.4729823141697265,1.044552555200692,0.7790980835277889,0.6033335558839198]
["Number of sq pixel of 1 arcmin",{"$nulls":5},148510660.4979094]
["Int time per sq pixel of 1 arcmin ","[s]",{"$nulls":4},0.6374815092909288]
["Unpol"]
["Sens unpol per pixel of diam FWHM","[W]",{"$nulls":4},4.752059256539316e-19,6.035529665095932e-19,6.256541249904714e-19,8.839075454651277e-19,7.809839509215942e-19,6.763034049566545e-19,1.346027571737e-18,1.7504065507306863e-18,1.789733292138215e-18,2.2566855757783655e-18,1.9706646118159337e-18,3.0643180973499116e-18,2.1990133544766394e-18,3.509974105503752e-18,5.793649784620567e-18,5.499269167309492e-18,9.326825654376674e-18,9.118605427914602e-18,1.5579244481438293e-17,2.0467631737348512e-17,2.581342638504773e-17,3.451654527999601e-17,8.608598455246006e-17,5.355036353038771e-17]
["Sens unpol per pixel of diam FWHM","[uK_CMB]",{"$nulls":4},1.7946877558157825,2.0190537199850005,2.662303557435332,2.49138711836197,3.633591032790143,5.9203193126056375,4.066219258458234,4.180564725732722,5.383744800498638,5.565678200049652,8.993833627647518,8.848488576827895,22.456733807762657,28.414223098287795,38.8946707487449,103.53784092788517,188.10096947985025,715.6274225751256,1860.2195267936925,8950.621406897151,43979.28536943319,492508.7392460609,2876937.9578696145,65971834.06473205]
["Sens per pixel of diam FWHM","[uK_RJ]",{"$nulls":4},1.6397720001860996,1.7851315188097996,2.266862771704606,2.0333736955719526,2.829651996092732,4.26152114024357,2.679621698791606,2.499331121197524,2.8948843364036856,2.669843922837463,3.6615841914082745,2.88379267584219,5.207476921655393,4.310948299562456,3.527980626367414,5.108945714705956,4.291155120486161,6.353543358357443,5.375860759640542,6.0537213065213,6.680493370871567,7.522402807016673,4.200750722317867,8.869625429463802]
["Sens unpol per sq pixel of 1 arcmin","[W]",{"$nulls":4},9.63131427174124e-18,1.0485093459393541e-17,9.510410925909055e-18,1.1943161056368052e-17,9.497232420443126e-18,7.151525486068753e-18,1.2591154725174033e-17,1.4679994227651654e-17,1.3602642719149087e-17,1.5681512963038606e-17,1.2289467447178286e-17,1.6938155763380248e-17,1.048679174343972e-17,1.4468944594597768e-17,2.072183825147809e-17,1.71472834620612e-17,2.520439643407946e-17,2.1324557949530245e-17,3.157549003845868e-17,3.555695085049961e-17,3.923833992643234e-17,4.4183353237391254e-17,9.516882837030158e-17,5.209635850233972e-17]
["Sens per pixel of diam 1 arcmin","[uK_CMB.arcmin]",{"$nulls":4},36.37412932534797,35.075574354322114,40.46900648358251,33.66306551065822,44.18664239965983,62.604023784972455,38.03666203037755,35.06080688309926,40.918475023039356,38.67541662824534,56.08738540773846,48.91041759483738,107.09306980808095,117.13015747409956,139.1124948973373,322.84157283918813,508.31564565379165,1673.5495974263526,3770.2305273919073,15549.27358135575,66851.80507640699,630442.2247965323,3180480.7271229043,64180559.97963205]
["Sens per pixel of diam 1 arcmin","[uK_RJ.arcmin]",{"$nulls":4},33.234348763772395,31.01181147410098,34.45801060111976,27.474490582857264,34.41026239290987,45.0631725650205,25.06600319552084,20.960939855289002,22.002204191170232,18.55251459691051,22.834387675916545,15.940293396744067,24.833740038457233,17.770749931955006,12.618340184799715,15.930215033501671,11.596225642548633,14.858248292593538,10.895614229971939,10.516696495267558,10.154849877441084,9.629149664899478,4.6439676167618975,8.628796439310927]
["Pol Q or U"]
["Sens pol per pixel of diam FWHM","[W]",{"$nulls":4},6.720426649798508e-19,8.535527908483812e-19,8.848085489161962e-19,1.2500340386806968e-18,1.1044780953890423e-18,9.564374475688044e-19,1.9035704472785897e-18,2.4754486837100456e-18,2.5310650947725124e-18,3.1914353472775016e-18,2.7869406209188044e-18,4.3336002126975635e-18,3.109874509740418e-18,4.963852983581779e-18,8.193458101050368e-18,7.777141039549281e-18,1.319012333430881e-17,1.289565546608575e-17,2.203237883717623e-17,2.8945602392616264e-17,3.6505697685054e-17,4.8813766461235397e-17,1.2174396688432977e-16,7.573165037468388e-17]
["Sens pol per pixel of diam FWHM","[uK_CMB]",{"$nulls":4},2.5380717644996134,2.855373153962637,3.7650657980791853,3.523353451909121,5.138673718689082,8.372595865466252,5.7505024228943045,5.912211333509775,7.613764913220807,7.871057594314495,12.719201493946334,12.513652551853417,31.758617517540348,40.18377966989346,55.00537087691115,146.42461885904333,266.0149421339319,1012.0500066118448,2630.7476837829013,12658.090185300907,62196.10183292905,696512.5386290536,4068604.6781251645,93298262.46897143]
["Sens per pixel of diam FWHM","[uK_RJ]",{"$nulls":4},2.318987801862839,2.5245572045205007,3.2058280757833195,2.8756246576505564,4.001732229670443,6.026700992872113,3.7895573484603227,3.534587968458693,4.09398469004353,3.775729485096128,5.178262023260506,4.078298713248224,7.3644844883499525,6.096601551930458,4.9893180495983245,7.225140319165069,6.068609769638282,8.985267186514598,7.602615195712984,8.561254774509397,9.447644328430124,10.63828407131642,5.940758643650502,12.543544575516998]
["Sens unpol per sq pixel of 1 arcmin","[W]",{"$nulls":4},1.3620735266574011e-17,1.482816137302378e-17,1.3449752115161851e-17,1.689018034352188e-17,1.3431114894000127e-17,1.0113784334055272e-17,1.78065817782792e-17,2.076064693230372e-17,1.9237041817536277e-17,2.2177008310858698e-17,1.737993153814219e-17,2.3954169602160353e-17,1.4830563109354647e-17,2.0462177678905047e-17,2.9305104692541896e-17,2.424992082990283e-17,3.564439926850325e-17,3.015747906383667e-17,4.465448625096483e-17,5.028512212941011e-17,5.5491392488966337e-17,6.248469737943992e-17,1.3458904779643789e-16,7.367537674425974e-17]
["Sens per pixel of diam 1 arcmin","[uK_CMB.arcmin]",{"$nulls":4},51.440787011420035,49.60435295990826,57.23181782484711,47.60676379622683,62.48934895732899,88.53545949583588,53.79196331076168,49.58346860182295,57.86746232920701,54.69529872609448,79.31954112167055,69.16977590395068,151.45247175875673,165.64705726276796,196.73477697937238,456.56693080704133,718.8668800500287,2366.7565379843813,5331.911145110702,21989.99358380297,94542.7294081773,891579.9445999237,4497878.979163454,90765018.36389554]
["Sens per pixel of diam 1 arcmin","[uK_RJ.arcmin]",{"$nulls":4},47.00046675836443,43.85732438043118,48.73098592449946,38.85479720156863,48.66345976087002,63.72894980501117,35.44868167359292,29.64324542343645,31.115815569255098,26.23721775907566,32.29270073976624,22.542979109881752,35.12021196683396,25.131635567311527,17.84502782398118,22.528726151897832,16.399539576030936,21.012736248492665,15.408725414411604,14.87285481496898,14.361126420539945,13.617674050221185,6.567561986846136,12.202960951430184]
[{"$nulls":6},47.00046675836443,43.85732438043117,48.73098592449946,38.85479720156863,48.66345976087001,63.72894980501117,35.448681673592915,29.64324542343645,31.115815569255098,26.23721775907566,32.29270073976624,22.542979109881752,35.12021196683397,25.131635567311527,17.845027823981184,22.528726151897835,16.399539576030936,21.012736248492665,15.408725414411602,14.872854814968978,14.361126420539943,13.617674050221186,6.567561986846136,12.202960951430185]
["CMB sensitivity"]
["CMB temp. Sens. Per FWHM pix","[µK]",{"$nulls":4},0.8026087640781265,0.9029482736220571,0.8418943064264556,0.6432733878914396,0.7267182065580285,0.8372595865466252,0.45461713366656986,0.3816316005657016,0.4721856551179852,0.454435722088452,0.6798699174812921,0.8848488576827894,2.8991518682559274,5.1877036483055186,8.697112775666623,26.733355574398125,59.48274936421445,226.30126114131963,588.2530652588687,10000000000000,10000000000000,10000000000000,10000000000000,10000000000000]
["CMB temp. Sens. Per pix of size max(FWHM)","[µK]",{"$nulls":4},0.8026087640781265,0.6633905683753889,0.47356554736488093,0.2858992835073064,0.2616185543608902,0.22791187233027224,0.09684151959761247,0.06534476870566114,0.06640110775096662,0.053419382841417985,0.06436638272012231,0.06581520429045537,0.1605066778273178,0.21460193201838387,0.27084434249480815,0.6327421437727364,1.0574710998082566,3.0128866128282183,5.882530652588683,73469387755.10197,56249999999.999985,39889196675.900246,29752066115.702465,23039999999.999985]
["Total temp. Sens. Per pix of size max(FWHM)","[µK]",null,null,0.025638270797518622]
["Cl noise unpol per et","[µK.arcmin]",{"$nulls":4},51.44078701142002,49.604352959908255,57.231817824847106,47.60676379622683,62.489348957328986,88.53545949583588,53.79196331076169,49.58346860182294,57.86746232920701,54.695298726094464,79.31954112167057,69.16977590395068,151.45247175875673,165.64705726276793,196.73477697937244,456.56693080704133,718.8668800500285,2366.7565379843813,5331.911145110701,0,0,0,0,0]
["Cl noisz unpol RJ per det","[µK_RJ.arcmin]",{"$nulls":4},47.00046675836442,43.857324380431166,48.730985924499464,38.85479720156863,48.663459760870026,63.72894980501116,35.44868167359293,27.177448038042638,28.527526210951432,24.05474205419932,29.60651520528812,20.66779917751896,32.19882715875123,23.041124883095,16.360634926978637,20.65473181531003,15.035385913683683,19.26484564605079,14.12699008832387,0,0,0,0,0]
["Cl noise unpol ","[µK.arcmin]",{"$nulls":4},16.267005158769326,15.68627372122251,12.797423513224228,8.691766140337903,8.837328479931967,8.853545949583587,4.252628096855469,2.934365500760803,3.2902635629226973,2.8951581722685886,3.8871302686328426,4.484192988031346,12.675604118742422,19.606091459141897,28.518985085125788,76.42346937510067,147.37248329466968,485.2008042606994,1093.0771857326426,15927214958824.645,13936313088971.568,11735842601239.217,10135500428342.96,8919240376941.803]
["Cl noise unpol RJ","[µK_RJ.arcmin]",{"$nulls":4},14.862852604746232,13.868903712299547,10.896579713776623,7.09388296486258,6.882052478581976,6.372894980501116,2.8024643534705787,1.754296727395943,1.7692020710310243,1.3888011800278988,1.5825348044928758,1.4614340950625404,2.9393373266763376,2.9745964316704083,2.586843516787753,3.771020844821644,3.36201449709395,4.307750444061042,3.158891015495793,10772315816.584894,2116938609.2383678,179249073.7553421,14799314.885797186,1199152.9776358756]
["Total uK arcmin unpol",null,null,null,1.333931561782168]
[]
["CMB Q&U Sens. Per FWHM pix","[µK]",{"$nulls":4},1.1350601994387943,1.2769616946776856,1.190618346232984,0.9097259494697627,1.0277347437378164,1.1840638625211277,0.6429257161184453,0.539708585350167,0.6677713574258796,0.6426691614042995,0.9614812579515204,1.2513652551853416,4.100019891466829,7.336520857006049,12.299574840836053,37.80667402105621,84.12131087811167,320.0383126881897,831.9154629966375,1e+20,1e+20,1e+20,1e+20,1e+20]
["CMB Q&U Sens. Per pix of size max(FWHM)","[µK]",{"$nulls":4},1.1350601994387943,0.9381759389468709,0.6697228197560539,0.40432264420878355,0.3699845077456138,0.3223160608753165,0.1369545904157635,0.09241145813367899,0.09390534713801436,0.07554641570793394,0.09102781140369427,0.09307675451791798,0.22699072063484188,0.3034929627718676,0.3830317424481815,0.8948325212084314,1.4954899711664291,4.260865109754005,8.319154629966379,7.3469387755102e+17,5.6249999999999994e+17,3.988919667590028e+17,2.975206611570249e+17,2.3039999999999994e+17]
["Total Q&U Sens. Per pix of size max(FWHM)","[µK]",null,null,0.036257990277644925]
["Cl noise pol per et","[µK.arcmin]",{"$nulls":4},72.74825865069594,70.15114870864424,80.93801296716504,67.32613102131644,88.37328479931968,125.20804756994494,76.07332406075511,70.12161376619854,81.83695004607873,77.35083325649066,112.17477081547696,97.82083518967477,214.1861396161619,234.2603149481991,278.2249897946747,645.6831456783764,1016.6312913075832,3347.099194852705,7540.461054783814,0,0,0,0,0]
["Cl noisz pol RJ per det","[µK_RJ.arcmin]",{"$nulls":4},66.46869752754478,62.023622948201954,68.91602120223955,54.94898116571453,68.82052478581976,90.12634513004102,50.13200639104169,41.92187971057801,44.00440838234047,37.10502919382102,45.668775351833105,31.88058679348814,49.667480076914465,35.54149986391002,25.236680369599434,31.860430067003353,23.19245128509727,29.716496585187073,21.791228459943877,0,0,0,0,0]
["Cl noise pol","[µK.arcmin]",{"$nulls":4},23.00501931472468,22.18374103964955,18.098289895834046,12.292013556641114,12.497869791465797,12.520804756994494,6.014124330301888,4.526330705427927,5.0753121892778434,4.465852440267674,5.9959937118771895,6.916977590395068,19.55243002878713,30.24287661572265,43.991233486413755,117.88507462964701,227.3256675417147,748.4341327125462,1686.0983500186373,1.73722838610667e+20,1.520074837843337e+20,1.280063021341757e+20,1.1055089729769721e+20,9.728478962197355e+19]
["Cl noise unpol RJ","[µK_RJ.arcmin]",{"$nulls":4},21.019247729184404,19.613591725180587,15.41009081470244,10.032265498796122,9.732691952174005,9.012634513004102,3.9632830967452386,2.7060456993463204,2.72903755722937,2.1422598593341484,2.4410987234300863,2.2542979109881753,4.533999868760746,4.5883879024052225,3.990269527479708,5.816892079837856,5.185989763832985,6.644810641761866,4.872666814966256,1.1749683085873373e+17,2.309007477529178e+16,1955122599375578.5,161420499321465.28,13079515768569.19]
["Total uK arcmin pol",null,null,null,2.021099628243735]
[]
["Focal plane area"]
["Horn beam waist","[mm]","wo",null,null,null,10.358996090355472,8.879139506018976,7.769247067766604,6.905997393570315,6.215397654213284,5.4046936123593765,4.781075118625602,4.286481140836748,3.884623533883302,3.5516558024075904,3.1873834124170686,2.8251807519151284,2.437410844789523,2.1069144590553504,1.8280581335921422,1.5936917062085343,1.381199478714063,1.1952687796564005,1.0358996090355472,0.8879139506018976,0.7769247067766605,0.6542523846540298,0.5650361503830257,0.49723181233706265]
[{"$nulls":6},32.19579204461685,27.59639318110016,24.14684403346264,21.463861363077903,19.317475226770114,16.797804545017488,14.8595963282847,13.32239670811732,12.07342201673132,11.038557272440064,9.906397552189802,8.780670557622777,7.575480481086319,6.548296687040716,5.681610360814739,4.953198776094901,4.29277227261558,3.714899082071175,3.2195792044616853,2.759639318110016,2.414684403346264,2.0334184449231696,1.7561341115245555,1.545398018141609]
[{"$nulls":6},3.2195792044616853,3.2195792044616858,3.2195792044616853,3.2195792044616853,3.2195792044616858,3.2195792044616853,3.2195792044616853,3.2195792044616858,3.2195792044616853,3.2195792044616858,3.2195792044616853,3.2195792044616853,3.2195792044616853,3.2195792044616858,3.2195792044616853,3.2195792044616853,3.2195792044616853,3.2195792044616853,3.2195792044616853,3.2195792044616858,3.2195792044616858,3.2195792044616853,3.2195792044616853,3.2195792044616853]
["Horn FWHM","[°]",null,10.38740589238607]
["Horn solid angle","[sr]",null,0.037236339817425364]
["filling factor",null,null,0.8]
["aperture efficiency",null,null,0.745]
["Total throughput","[m^2 sr]",{"$nulls":4},0.000125,9.183673469387756e-05,0.000140625,0.0001666666666666667,0.000225,0.00034026465028355395,0.0004260355029585798,0.0005136741973840667,0.00045703124999999997,0.0004408163265306122,0.0004142011834319528,0.00018595041322314046,8.304498269896194e-05,3.102556736569951e-05,1.5570934256055366e-05,8.875739644970416e-06,4.444444444444444e-06,3.3284023668639047e-06,2.4999999999999998e-06,0,0,0,0,0]
["focal plane area ","[m^2]",{"$nulls":4},0.0033569357410768975,0.0024663201363013944,0.0037765527087115095,0.004475914321435864,0.006042484333938415,0.00913797252769515,0.01144139045479463,0.013794970179740499,0.012273796303312406,0.01183833665424669,0.011123574053272562,0.004993788705734227,0.0022302133643140637,0.0008332066878168455,0.000418165005808887,0.0002383623011415549,0.00011935771523828969,8.938586292808305e-05,6.713871482153795e-05,0,0,0,0,0]
["focal plane area (including efficiency effects)","[m^2]",{"$nulls":4},0.005632442518585398,0.004138121034062742,0.006336497833408573,0.007509923358113865,0.010138396533453716,0.015332168670629445,0.01919696385032656,0.023145923120369963,0.020593617958577864,0.019862980963501156,0.018663714854484162,0.008378840110292328,0.0037419687320705765,0.001397997798350412,0.0007016191372632331,0.00039993674688180357,0.00020026462288303637,0.00014997628008067625,0.00011264885037170796,0,0,0,0,0]
["Equivalent diameter","[m]",{"$nulls":4},0.09555611903215848,0.08190524488470728,0.10135256962726229,0.11033870209186526,0.1282019866931807,0.15765651156927932,0.1764112966747541,0.19370791732091644,0.18271594334556415,0.17944540080535518,0.17394388429465027,0.11654726063016425,0.07788614265308136,0.04760618307039471,0.033725689070173585,0.025462777405815065,0.01801823460040218,0.01559270301957881,0.013513675950301637,0,0,0,0,0]
["total FP area","[m^2]",{"$nulls":4},0.16563400297370723]
["FP diameter","[m]",null,null,0.4592295314316203]
["FOV","[°]",null,null,13.09860812262234]
[]
[]
["Far sidelobes"]
["Earth RJ temperature","[K]",null,300]
["Earth solid angle","[sr]",null,5.541769440932395e-05]
["Moon RJ temperature","[K]",null,200]
["Moon solid angle","[sr]",null,7.77063855613958e-06]
["Sun RJ temperature","[K]",null,6000]
["Sun solid angle","[sr]",null,6.665602685452734e-05]
["Sidelobe signal","[Kcmb]",null,6e-09]
[]
["dTrj/dTcmb",{"$nulls":5},0.9119823548667598,0.8824989819403023,0.8498837526192877,0.814643985711614,0.7773003285236163,0.7184745437767771,0.6577707574313655,0.5967339052433085,0.5367086814224337,0.4788060730876327,0.4063647648314133,0.32530205667309414,0.23145823228677403,0.15143591902975564,0.09053738805942152,0.04925202064140435,0.02277063014549724,0.008861778546432513,0.0028845341289748666]
["Earth rejection factor wrt main beam","dB",{"$nulls":4},-107.8246421031772,-109.30630012158373,-110.62968592333759,-111.8366530847656,-112.95559293924762,-114.51132440606487,-115.95960287686884,-117.33103435352618,-118.64649490309208,-119.92064592275963,-121.57301323905071,-123.58706697776176,-126.34755874083879,-129.4556327960949,-132.9227801802136,-136.7585330642503,-141.35198123457434,-146.70633939529375,-152.82374964179354]
["Moon rejection factor wrt main beam","dB",{"$nulls":4},-97.53181206407378,-99.01347008248032,-100.33685588423417,-101.54382304566218,-102.6627629001442,-104.21849436696147,-105.66677283776544,-107.03820431442276,-108.35366486398867,-109.62781588365623,-111.28018319994729,-113.29423693865834,-116.0547287017354,-119.16280275699148,-122.6299501411102,-126.46570302514687,-131.05915119547095,-136.41350935619033,-142.53091960269012]
["Sun rejection factor wrt main beam","dB",{"$nulls":4},-121.63685175728973,-123.11850977569627,-124.44189557745013,-125.64886273887814,-126.76780259336016,-128.32353406017742,-129.77181253098138,-131.1432440076387,-132.4587045572046,-133.73285557687217,-135.38522289316325,-137.3992766318743,-140.15976839495133,-143.26784245020744,-146.73498983432614,-150.5707427183628,-155.16419088868687,-160.5185490494063,-166.6359592959061]
[]
["Integrated galactic emission (from PSM)","[uK_RJ.arcmin^2]",{"$nulls":4},9833140,8047570,7389060,7343760,7653690,8506200,9635460,10938200,12360900,13871500,15985500,18738900,22713600,27316000,32446000,37781500,43666200,49769600,55612300]
["Galactic rejection factor","dB",{"$nulls":4},-64.81838959025882,-65.42977301351303,-66.38240311631753,-67.56266310012478,-68.86112687997651,-70.875505565548,-72.86515266738128,-74.78731821545203,-76.63382109500101,-78.40870544694585,-80.67710074943066,-83.38133317579059,-86.97724373620132,-90.88662909860628,-95.10121708074249,-99.59815028904626,-104.82026049258431,-110.74280616052393,-117.34228347278189]

{"sheet":"COrE+ Extended","index":1,"n_rows":131,"n_cols":30,"rows_kept":131,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["COrE+ EXTENDED sensitivity estimate","V0.91"]
["M. Piat, J. Delabrouille"]
["2014-10-07"]
[{"$nulls":17},"Core channels"]
["nu (GHz)","[GHz]","nu",null,null,null,60,70,80,90,100,115,130,145,160,175,195,220,255,295,340,390,450,520,600,700,800,950,1100,1250]
["Number of detectors (2 x nb of horns)",{"$nulls":5},20,40,80,130,200,360,600,650,700,700,700,450,250,230,150,130,90,70,50,40,40,40,40,40]
["Scaling factor",null,null,null,1]
["Total number of detectors",null,null,null,5800]
[]
["Parameter","Units","Formula","Values"]
[]
["Mission duration","[yr]","tmiss",3]
[]
["Rotation speed","[rpm]","w",2]
["Boresight angle","[°]","b",45]
["Scanning speed","[°/s]","ss=2pi*sin(b)/60*w",8.48528137423857]
[]
["Telescope diameter","m","Dtel",1.5]
["Telescope f number",null,"f#=F/D",2]
["Telescope temperature","[K]","Ttel",40]
["Telescope emissivity","[%]","e_tel",0.5]
["Payload enclosure temperature","[K]",null,40]
[]
["Lambda center","[mm]","la",null,null,null,5,4.285714285714286,3.75,3.3333333333333335,3,2.608695652173913,2.3076923076923075,2.0689655172413794,1.875,1.7142857142857142,1.5384615384615385,1.3636363636363635,1.1764705882352942,1.0169491525423728,0.8823529411764706,0.7692307692307693,0.6666666666666666,0.5769230769230769,0.5,0.42857142857142855,0.375,0.3157894736842105,0.2727272727272727,0.24]
["dnu/nu",{"$nulls":5},0.35,0.35,0.25,0.35,0.2,0.1,0.28,0.35,0.28,0.35,0.2,0.35,0.12,0.2,0.35,0.2,0.35,0.2,0.35,0.35,0.35,0.35,1.35,0.35]
["dnu","[GHz]","dnu",null,null,null,21,24.5,20,31.499999999999996,20,11.5,36.400000000000006,50.75,44.800000000000004,61.24999999999999,39,77,30.599999999999998,59,118.99999999999999,78,157.5,104,210,244.99999999999997,280,332.5,1485,437.5]
["Beam étendue","[m^2.sr]","Aomega=la^2",null,null,null,2.5e-05,1.836734693877551e-05,1.40625e-05,1.1111111111111113e-05,9e-06,6.805293005671079e-06,5.3254437869822475e-06,4.2806183115338884e-06,3.515625e-06,2.938775510204081e-06,2.3668639053254444e-06,1.8595041322314046e-06,1.3840830449826992e-06,1.0341855788566503e-06,7.785467128027683e-07,5.917159763313611e-07,4.4444444444444444e-07,3.3284023668639047e-07,2.5e-07,1.8367346938775507e-07,1.40625e-07,9.97229916897507e-08,7.43801652892562e-08,5.76e-08]
["Airy disk diameter (first zeros)","[arcmin]","1,22*la/Dtel",null,null,null,13.980170201192086,11.983003029593217,10.485127650894066,9.32011346746139,8.388102120715251,7.294001844100219,6.452386246704039,5.784898014286382,5.242563825447033,4.793201211837287,4.301590831136027,3.812773691234206,3.2894518120451974,2.843424447700085,2.4670888590338977,2.1507954155680133,1.8640226934922781,1.6130965616760098,1.3980170201192086,1.1983003029593218,1.0485127650894064,0.8829581179700265,0.7625547382468411,0.6710481696572201]
["Edge taper","dB","EdB",null,null,null,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23,-23]
["Spill over (assuming gaussian beam)","%",{"$nulls":4},0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721,0.5011872336272721]
["Pure gaussian beam FWHM","[arcmin]","FWHM=2.355*la/(2*pi*Dtel/(sqrt(-2*EdB/10*ln(10)))",null,null,null,13.978173649525361,11.981291699593164,10.483630237144022,9.318782433016908,8.386904189715217,7.292960164969754,6.451464761319397,5.784071854976012,5.241815118572011,4.7925166798372665,4.300976507546265,3.81222917714328,3.288982035182438,2.843018369394988,2.466736526386828,2.1504882537731325,1.8637564866033813,1.6128661903298493,1.3978173649525363,1.1981291699593166,1.0483630237144022,0.8828320199700229,0.762445835428656,0.6709523351772173]
["Beam FWHM (Goldsmith)","[arcmin]","FWHM=(1.02-0.0135*EdB)*la/Dtel",null,null,null,15.246406928431208,13.068348795798176,11.434805196323403,10.164271285620805,9.147844157058723,7.954647093094545,7.03680319773748,6.308858039350844,5.717402598161701,5.22733951831927,4.691202131824986,4.158110980481238,3.5873898655132255,3.100964121036855,2.690542399134919,2.345601065912493,2.032854257124161,1.75920079943437,1.5246406928431209,1.3068348795798175,1.1434805196323403,0.9629309639009181,0.8316221960962475,0.7318275325646979]
[null,"[arcsec]","FWHM",{"$nulls":20},105.55204796606219,91.47844157058725,78.41009277478905,68.60883117794042,57.77585783405509,49.89733176577485,43.90965195388188]
["Polarisation efficiency",null,"eta_pol",null,null,null,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,2,1]
[]
["Bolometer performances"]
["Detection efficiency","[%]","eff",null,null,null,50,50,50,50,50,50,50,50,50,50,50,50,50,50,50,50,50,50,50,50,50,50,50,50]
["Power per mode","[W]","Pmode=eff*e_tel*bnu*Aomega*dnu/2",null,null,null,2.7892389032181035e-13,2.9922683448777037e-13,2.245687675544732e-13,3.251966058560068e-13,1.899037203851935e-13,9.644169680064372e-14,2.7026939369821647e-13,3.347865305058596e-13,2.637451799394302e-13,3.235368806765153e-13,1.8002096453530662e-13,3.0562006179904314e-13,1.0181641832965926e-13,1.6838386023880023e-13,3.006625620182054e-13,1.7989261806570944e-13,3.3742526617831547e-13,2.0930264926166978e-13,3.9813517887979943e-13,4.3315845764427337e-13,4.61881167781848e-13,4.935368034593584e-13,1.9785748184504547e-12,5.219496982919094e-13]
["Shot noise","[W/sqrt(Hz)]",{"$nulls":4},4.707198088795989e-18,5.266150683404963e-18,4.877122497884363e-18,6.2249841408474104e-18,5.014304795183438e-18,3.831998532732759e-18,6.820466849368672e-18,8.017001816546815e-18,7.47474273258745e-18,8.658146178758396e-18,6.817463797023456e-18,9.435094678953958e-18,5.8630418006747624e-18,8.109708264300918e-18,1.1633841107652938e-17,9.637912235770241e-18,1.417878604073848e-17,1.2004194598709003e-17,1.7784222954689716e-17,2.0036248614566365e-17,2.211842066953546e-17,2.4915268238395123e-17,5.3680502657773635e-17,2.939092973475167e-17]
["Photon NEP","[W/sqrt(Hz)]","NEPphot",null,null,null,5.437563634985991e-18,5.9195828622795395e-18,5.369305075655816e-18,6.7427659833954344e-18,5.36186486967113e-18,4.037546052444682e-18,7.108604612453434e-18,8.287903449302738e-18,7.679661705814103e-18,8.853332185365847e-18,6.9382806332244796e-18,9.562796646862371e-18,5.920541664714059e-18,8.168750883256995e-18,1.1698955194193688e-17,9.680864143917503e-18,1.4229678902061597e-17,1.2039233438652389e-17,1.7826615511212568e-17,2.0074434024330357e-17,2.2152840646805515e-17,2.4944653248444426e-17,5.372958930941612e-17,2.94121089308305e-17]
["Bolometer NEP","[W/sqrt(Hz)]","NEPphot",null,null,null,5.437563634985991e-18,5.9195828622795395e-18,5.369305075655816e-18,6.7427659833954344e-18,5.36186486967113e-18,4.037546052444682e-18,7.108604612453434e-18,8.287903449302738e-18,7.679661705814103e-18,8.853332185365847e-18,6.9382806332244796e-18,9.562796646862371e-18,5.920541664714059e-18,8.168750883256995e-18,1.1698955194193688e-17,9.680864143917503e-18,1.4229678902061597e-17,1.2039233438652389e-17,1.7826615511212568e-17,2.0074434024330357e-17,2.2152840646805515e-17,2.4944653248444426e-17,5.372958930941612e-17,2.94121089308305e-17]
["Total NEP","[W/sqrt(Hz)]",{"$nulls":4},7.689876238863935e-18,8.371554367427071e-18,7.593344058511152e-18,9.535711101625783e-18,7.582822018300759e-18,5.709952386073221e-18,1.0053085052479585e-17,1.1720865461642687e-17,1.0860681738799602e-17,1.2520502448738614e-17,9.812210571056646e-18,1.3523836712208722e-17,8.372910318833605e-18,1.1552358286749242e-17,1.654482110122388e-17,1.3690809367819535e-17,2.0123804891509802e-17,1.702604720951788e-17,2.5210641427167398e-17,2.8389536854171904e-17,3.132884768780233e-17,3.527706693264419e-17,7.598511390211274e-17,4.1595003347975325e-17]
["NET per bolo","[μKCMB.sqrt(s)]",{"$nulls":4},41.07157907910982,39.60532533860055,45.69527933374297,38.0104014256849,49.89302043013546,70.68887039347355,42.94881558573445,39.58865075769985,46.202793410485675,43.67006061523924,63.330656371454,55.22683625141123,120.92334763823648,132.25665093497176,157.0778446396144,364.5341740083578,573.9608514304623,1889.6761491857726,4257.127912731676,17557.34725103984,75485.22121912311,711859.1749355365,3591216.287961648,72469004.5765045]
[]
["Beam duration","[ms]","∆t_beam=FWHM/ss",null,null,null,29.946771466175747,25.668661256722064,22.460078599631803,19.96451431078383,17.968062879705446,15.624402504091696,13.82158683054265,12.391767503245136,11.230039299815902,10.267464502688824,9.214391220361765,8.167301308957022,7.046299168511941,6.090868772781507,5.284724376383956,4.607195610180883,3.9929028621567664,3.4553967076356624,2.9946771466175752,2.566866125672206,2.2460078599631808,1.8913750399689941,1.6334602617914042,1.437445030376436]
["Required time constant","[ms]","tau=tbeam/(3pi)",null,null,null,3.177451138990131,2.723529547705826,2.3830883542425974,2.1183007593267535,1.9064706833940783,1.6578005942557206,1.466515910303137,1.314807367857985,1.1915441771212987,1.0894118190823303,0.9776772735354246,0.8665775833609448,0.7476355621153249,0.646261248608162,0.5607266715864937,0.4888386367677123,0.4236601518653508,0.3666289775757843,0.31774511389901317,0.2723529547705826,0.2383088354242598,0.2006811245677977,0.17331551667218895,0.15251765467152628]
[null,"[µs]","tau",null,null,null,3177.451138990131,2723.529547705826,2383.0883542425972,2118.3007593267535,1906.4706833940784,1657.8005942557206,1466.5159103031372,1314.8073678579851,1191.5441771212986,1089.4118190823303,977.6772735354245,866.5775833609448,747.6355621153249,646.2612486081621,560.7266715864937,488.8386367677123,423.66015186535077,366.6289775757843,317.7451138990132,272.3529547705826,238.3088354242598,200.6811245677977,173.31551667218895,152.5176546715263]
[]
["Sampling"]
["Number of sample per beam",null,"Nsbeam",null,null,null,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["Sampling frequency","[Hz]","fsamp",null,null,null,133.57032508555778,155.83204593315077,178.09376678074375,200.35548762833665,222.61720847592963,256.009789747319,289.4023710187086,322.79495229009797,356.1875335614875,389.580114832877,434.1035565280629,489.7578586470451,567.6738816136206,656.7207650039925,756.8985088181606,868.2071130561258,1001.7774381416833,1157.6094840748344,1335.7032508555776,1558.320459331508,1780.937667807437,2114.863480521332,2448.789293235226,2782.7151059491202]
["Coding in bits per bolometer","[bits]","Nbits",null,null,null,16,16,16,16,16,16,16,16,16,16,16,16,16,16,16,16,16,16,16,17,18,19,20,20]
["Data rate per bolometer","[kbits/s]","fsamp*Nbits/1000",null,null,null,2.1371252013689244,2.493312734930412,2.8495002684919,3.2056878020533865,3.5618753356148742,4.096156635957104,4.630437936299337,5.1647192366415675,5.6990005369838,6.2332818373260315,6.945656904449006,7.836125738352722,9.082782105817929,10.50753224006388,12.11037614109057,13.891313808898012,16.028439010266933,18.52175174519735,21.37125201368924,26.491447808635634,32.056878020533865,40.18240612990531,48.97578586470452,55.65430211898241]
["Data rate per channel","[kbits/s]",{"$nulls":4},42.74250402737849,99.73250939721649,227.960021479352,416.73941426694023,712.3750671229749,1474.6163889445577,2778.2627617796024,3357.067503817019,3989.3003758886603,4363.297286128222,4861.959833114304,3526.256582258725,2270.695526454482,2416.732415214692,1816.5564211635856,1805.8707951567415,1442.559510924024,1296.5226221638145,1068.562600684462,1059.6579123454253,1282.2751208213547,1607.2962451962123,1959.0314345881807,2226.1720847592965]
[]
["Total data rate","[kbits/s]",{"$nulls":4},46102.24293769723]
["Compression factor",{"$nulls":5},4]
["Total data rate with compresion","[kbits/s]",{"$nulls":4},11525.560734424307]
[]
["Sensitivity per horn"]
["Number of pixel of diam FWHM",null,"Npix",null,null,null,813453.5041416222,1107200.6028594305,1446139.56291844,1830270.3843186502,2259593.067060062,2988311.83118693,3818712.283331505,4750794.42349378,5784558.25167376,6920003.767871441,8592102.637495888,10936430.444570698,14693003.91855805,19664108.66609019,26120895.855214313,34368410.54998355,45756759.607966244,61099396.53330408,81345350.41416222,110720060.28594306,144613956.29184398,203928274.30217066,273410761.1142675,353061416.72813475]
["int time per pixel of diam FWHM","[s]","tint",null,null,null,116.38378778625001,85.50645633275509,65.4658806297656,51.726127905,41.898163603049994,31.68103107981098,24.79181278286982,19.927782926539834,16.3664701574414,13.681033013240812,11.01858345905325,8.656645372530992,6.443393095432527,4.8144973976501,3.624408616180796,2.7546458647633125,2.0690451162000003,1.5494882989293637,1.1638378778625,0.8550645633275508,0.6546588062976562,0.4642455800891965,0.3462658149012396,0.26814824705951995]
["Number of sq pixel of 1 arcmin",{"$nulls":5},148510660.4979094]
["Int time per sq pixel of 1 arcmin ","[s]",{"$nulls":4},0.6374815092909288]
["Unpol"]
["Sens unpol per pixel of diam FWHM","[W]",{"$nulls":4},7.128088884808974e-19,9.0532944976439e-19,9.38481187485707e-19,1.3258613181976915e-18,1.1714759263823912e-18,1.0144551074349816e-18,2.0190413576054998e-18,2.6256098260960293e-18,2.684599938207322e-18,3.3850283636675473e-18,2.9559969177239005e-18,4.5964771460248664e-18,3.2985200317149595e-18,5.264961158255628e-18,8.690474676930848e-18,8.248903750964238e-18,1.399023848156501e-17,1.3677908141871905e-17,2.3368866722157437e-17,3.070144760602276e-17,3.8720139577571595e-17,5.177481791999401e-17,1.2912897682869007e-16,8.032554529558156e-17]
["Sens unpol per pixel of diam FWHM","[uK_CMB]",{"$nulls":4},2.6920316337236736,3.028580579977501,3.9934553361529974,3.7370806775429544,5.450386549185215,8.880478968908454,6.09932888768735,6.2708470885990835,8.075617200747955,8.348517300074475,13.490750441471278,13.27273286524184,33.68510071164399,42.62133464743169,58.34200612311733,155.30676139182776,282.15145421977536,1073.4411338626885,2790.3292901905384,13425.932110345724,65968.92805414977,738763.1088690914,4315406.936804421,98957751.09709808]
["Sens per pixel of diam FWHM","[uK_RJ]",{"$nulls":4},2.4596580002791493,2.6776972782147,3.400294157556909,3.0500605433579286,4.244477994139098,6.392281710365354,4.019432548187409,3.7489966817962865,4.342326504605528,4.004765884256194,5.492376287112411,4.325689013763284,7.811215382483091,6.466422449343685,5.29197093955112,7.663418572058934,6.436732680729242,9.530315037536166,8.063791139460813,9.080581959781947,10.02074005630735,11.283604210525008,6.3011260834768,13.304438144195702]
["Sens unpol per sq pixel of 1 arcmin","[W]",{"$nulls":4},9.63131427174124e-18,1.0485093459393541e-17,9.510410925909055e-18,1.1943161056368052e-17,9.497232420443126e-18,7.151525486068753e-18,1.2591154725174033e-17,1.4679994227651654e-17,1.3602642719149087e-17,1.5681512963038606e-17,1.2289467447178286e-17,1.6938155763380248e-17,1.048679174343972e-17,1.4468944594597768e-17,2.072183825147809e-17,1.71472834620612e-17,2.520439643407946e-17,2.1324557949530245e-17,3.157549003845868e-17,3.555695085049961e-17,3.923833992643234e-17,4.4183353237391254e-17,9.516882837030158e-17,5.209635850233972e-17]
["Sens per pixel of diam 1 arcmin","[uK_CMB.arcmin]",{"$nulls":4},36.37412932534797,35.075574354322114,40.46900648358251,33.66306551065822,44.18664239965983,62.604023784972455,38.03666203037755,35.06080688309926,40.918475023039356,38.67541662824534,56.08738540773846,48.91041759483738,107.09306980808095,117.13015747409956,139.1124948973373,322.84157283918813,508.31564565379165,1673.5495974263526,3770.2305273919073,15549.27358135575,66851.80507640699,630442.2247965323,3180480.7271229043,64180559.97963205]
["Sens per pixel of diam 1 arcmin","[uK_RJ.arcmin]",{"$nulls":4},33.234348763772395,31.01181147410098,34.45801060111976,27.474490582857264,34.41026239290987,45.0631725650205,25.06600319552084,20.960939855289002,22.002204191170232,18.55251459691051,22.834387675916545,15.940293396744067,24.833740038457233,17.770749931955006,12.618340184799715,15.930215033501671,11.596225642548633,14.858248292593538,10.895614229971939,10.516696495267558,10.154849877441084,9.629149664899478,4.6439676167618975,8.628796439310927]
["Pol Q or U"]
["Sens pol per pixel of diam FWHM","[W]",{"$nulls":4},1.0080639974697763e-18,1.280329186272572e-18,1.3272128233742942e-18,1.8750510580210452e-18,1.6567171430835633e-18,1.4346561713532062e-18,2.8553556709178844e-18,3.713173025565068e-18,3.796597642158768e-18,4.787153020916251e-18,4.180410931378206e-18,6.500400319046343e-18,4.664811764610628e-18,7.44577947537267e-18,1.2290187151575547e-17,1.1665711559323922e-17,1.9785185001463215e-17,1.934348319912863e-17,3.3048568255764346e-17,4.341840358892438e-17,5.4758546527580996e-17,7.32206496918531e-17,1.8261595032649465e-16,1.1359747556202582e-16]
["Sens pol per pixel of diam FWHM","[uK_CMB]",{"$nulls":4},3.8071076467494205,4.283059730943957,5.647598697118777,5.285030177863682,7.708010578033623,12.558893798199376,8.625753634341455,8.868317000264662,11.42064736983121,11.806586391471738,19.0788022409195,18.77047882778012,47.63792627631053,60.27566950484021,82.50805631536669,219.63692828856503,399.0224132008978,1518.0750099177674,3946.1215256743517,18987.13527795135,93294.15274939359,1044768.8079435807,6102907.017187747,139947393.70345715]
["Sens per pixel of diam FWHM","[uK_RJ]",{"$nulls":4},3.4784817027942596,3.7868358067807515,4.808742113674978,4.313436986475835,6.002598344505663,9.040051489308167,5.684336022690484,5.3018819526880385,6.140977035065293,5.66359422764419,7.767393034890758,6.117448069872334,11.046726732524931,9.144902327895688,7.483977074397483,10.837710478747603,9.102914654457424,13.477900779771899,11.403922793569476,12.84188216176409,14.171466492645187,15.957426106974628,8.911137965475755,18.8153168632755]
["Sens unpol per sq pixel of 1 arcmin","[W]",{"$nulls":4},1.3620735266574011e-17,1.482816137302378e-17,1.3449752115161851e-17,1.689018034352188e-17,1.3431114894000127e-17,1.0113784334055272e-17,1.78065817782792e-17,2.076064693230372e-17,1.9237041817536277e-17,2.2177008310858698e-17,1.737993153814219e-17,2.3954169602160353e-17,1.4830563109354647e-17,2.0462177678905047e-17,2.9305104692541896e-17,2.424992082990283e-17,3.564439926850325e-17,3.015747906383667e-17,4.465448625096483e-17,5.028512212941011e-17,5.5491392488966337e-17,6.248469737943992e-17,1.3458904779643789e-16,7.367537674425974e-17]
["Sens per pixel of diam 1 arcmin","[uK_CMB.arcmin]",{"$nulls":4},51.440787011420035,49.60435295990826,57.23181782484711,47.60676379622683,62.48934895732899,88.53545949583588,53.79196331076168,49.58346860182295,57.86746232920701,54.69529872609448,79.31954112167055,69.16977590395068,151.45247175875673,165.64705726276796,196.73477697937238,456.56693080704133,718.8668800500287,2366.7565379843813,5331.911145110702,21989.99358380297,94542.7294081773,891579.9445999237,4497878.979163454,90765018.36389554]
["Sens per pixel of diam 1 arcmin","[uK_RJ.arcmin]",{"$nulls":4},47.00046675836443,43.85732438043118,48.73098592449946,38.85479720156863,48.66345976087002,63.72894980501117,35.44868167359292,29.64324542343645,31.115815569255098,26.23721775907566,32.29270073976624,22.542979109881752,35.12021196683396,25.131635567311527,17.84502782398118,22.528726151897832,16.399539576030936,21.012736248492665,15.408725414411604,14.87285481496898,14.361126420539945,13.617674050221185,6.567561986846136,12.202960951430184]
[{"$nulls":6},47.00046675836443,43.85732438043117,48.73098592449946,38.85479720156863,48.66345976087001,63.72894980501117,35.448681673592915,29.64324542343645,31.115815569255098,26.23721775907566,32.29270073976624,22.542979109881752,35.12021196683397,25.131635567311527,17.845027823981184,22.528726151897835,16.399539576030936,21.012736248492665,15.408725414411602,14.872854814968978,14.361126420539943,13.617674050221186,6.567561986846136,12.202960951430185]
["CMB sensitivity"]
["CMB temp. Sens. Per FWHM pix","[µK]",{"$nulls":4},0.8512951495790957,0.677211205216543,0.6314207298198417,0.46352780997749965,0.5450386549185213,0.6619118215745514,0.35214491751823523,0.34784401105443186,0.4316598964562469,0.44624702034905295,0.7211109434636401,0.8848488576827893,3.012887000806499,3.9744599492349533,6.736754588048917,19.26343292914488,42.06065543905583,181.44466829693084,558.0658580381075,3002.1296860030243,14751.100753187184,165192.4530700366,964954.3261268822,22127625.835361566]
["CMB temp. Sens. Per pix of size max(FWHM)","[µK]",{"$nulls":4},0.8512951495790957,0.4975429262815416,0.35517416052366074,0.2060123599899998,0.19621391577066757,0.18018015558929196,0.07501311852459445,0.05955949773107987,0.06070217293915969,0.05245679259613354,0.06827085855277064,0.0658152042904554,0.166803432570602,0.16441316652968482,0.20979512557937802,0.4559392409265059,0.7477449855832147,2.4156834536573624,5.580658580381075,22.05646299920588,82.97494173667786,658.9394249885114,2870.938490956012,50982.04992467304]
["Total temp. Sens. Per pix of size max(FWHM)","[µK]",null,null,0.024014772180477425]
["Cl noise unpol per et","[µK.arcmin]",{"$nulls":4},51.44078701142001,49.604352959908255,57.231817824847106,47.60676379622683,62.48934895732896,88.53545949583587,53.79196331076169,49.58346860182294,57.867462329207,54.695298726094464,79.31954112167054,69.16977590395066,151.45247175875664,165.64705726276796,196.73477697937238,456.5669308070413,718.8668800500284,2366.7565379843813,5331.911145110702,21989.993583802967,94542.72940817727,891579.9445999237,4497878.979163453,90765018.36389555]
["Cl noisz unpol RJ per det","[µK_RJ.arcmin]",{"$nulls":4},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"}]
["Cl noise unpol ","[µK.arcmin]",{"$nulls":4},11.502509657362339,7.843136860611255,6.398711756612114,4.175389396073629,4.418664239965982,4.666228428273736,2.19604770623133,1.7830484760195866,2.0052491549891025,1.8953259247558305,2.7486161723057685,2.9894619920208965,8.78191614011648,10.01388803834872,14.727140571390647,36.71264717524345,69.47205486530808,259.35073904724334,691.3227130564114,3187.7043228825946,13705.063900225397,129244.84187616972,652019.6657193605,13157440.9197745]
["Cl noise unpol RJ","[µK_RJ.arcmin]",{"$nulls":4},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"}]
["Total uK arcmin unpol",null,null,null,0.8099735226972005]
[]
["CMB Q&U Sens. Per FWHM pix","[µK]",{"$nulls":4},1.2039131461171897,0.9577212710082644,0.8929637596747378,0.6555273154072789,0.7708010578033622,0.9360846751658108,0.4980081182750432,0.4919257180234344,0.6104592799009904,0.6310885883462133,1.019804876221938,1.2513652551853414,4.260865658438149,5.620735163316754,9.52720970479795,27.24260810626117,59.48274936421444,256.60151072580715,789.2243051348701,4245.652517948359,20861.206745089294,233617.4075333268,682325.7475396137,31293188.559485614]
["CMB Q&U Sens. Per pix of size max(FWHM)","[µK]",{"$nulls":4},1.2039131461171897,0.7036319542101532,0.5022921148170401,0.29134547351434625,0.27748838080921046,0.25481321970487103,0.10608456957338198,0.08422984945942279,0.08584583623607678,0.07418510752804466,0.09654957408018348,0.09307675451791793,0.2358956765917315,0.23251532993898658,0.2966951119141229,0.644795458136359,1.0574710998082566,3.4162923025625216,7.892243051348703,31.19254911145733,117.34428794112729,931.8810716010821,2030.06007532447,72099.50644105485]
["Total Q&U Sens. Per pix of size max(FWHM)","[µK]",null,null,0.0339620165149313]
["Cl noise pol per et","[µK.arcmin]",{"$nulls":4},72.74825865069593,70.15114870864424,80.93801296716504,67.32613102131644,88.37328479931965,125.2080475699449,76.07332406075511,70.12161376619855,81.83695004607873,77.35083325649067,112.1747708154769,97.82083518967475,214.18613961616185,234.2603149481991,278.22498979467457,645.6831456783763,1016.6312913075831,3347.099194852705,7540.461054783815,31098.547162711504,133703.61015281398,1260884.4495930648,3180480.7271229043,128361119.95926411]
["Cl noisz pol RJ per det","[µK_RJ.arcmin]",{"$nulls":4},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"}]
["Cl noise pol","[µK.arcmin]",{"$nulls":4},16.267005158769322,11.091870519824777,9.049144947917023,5.904892312116133,6.248934895732896,6.599043528395608,3.105680449770673,2.750395976295868,3.09314596968486,2.9235866928614107,4.239807813620257,4.6113183935967115,13.546320888517883,15.446667736838968,22.716975289600327,56.630158084860874,107.16234737100339,400.0548715968067,1066.3822290221403,4917.112047816766,21140.396973505285,199363.33635009258,502878.1575988421,20295675.10406872]
["Cl noise unpol RJ","[µK_RJ.arcmin]",{"$nulls":4},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"}]
["Total uK arcmin pol",null,null,null,1.2186924260926704]
[]
["Focal plane area"]
["Horn beam waist","[mm]","wo",null,null,null,10.358996090355472,8.879139506018976,7.769247067766604,6.905997393570315,6.215397654213284,5.4046936123593765,4.781075118625602,4.286481140836748,3.884623533883302,3.5516558024075904,3.1873834124170686,2.8251807519151284,2.437410844789523,2.1069144590553504,1.8280581335921422,1.5936917062085343,1.381199478714063,1.1952687796564005,1.0358996090355472,0.8879139506018976,0.7769247067766605,0.6542523846540298,0.5650361503830257,0.49723181233706265]
[{"$nulls":6},32.19579204461685,27.59639318110016,24.14684403346264,21.463861363077903,19.317475226770114,16.797804545017488,14.8595963282847,13.32239670811732,12.07342201673132,11.038557272440064,9.906397552189802,8.780670557622777,7.575480481086319,6.548296687040716,5.681610360814739,4.953198776094901,4.29277227261558,3.714899082071175,3.2195792044616853,2.759639318110016,2.414684403346264,2.0334184449231696,1.7561341115245555,1.545398018141609]
[{"$nulls":6},3.2195792044616853,3.2195792044616858,3.2195792044616853,3.2195792044616853,3.2195792044616858,3.2195792044616853,3.2195792044616853,3.2195792044616858,3.2195792044616853,3.2195792044616858,3.2195792044616853,3.2195792044616853,3.2195792044616853,3.2195792044616858,3.2195792044616853,3.2195792044616853,3.2195792044616853,3.2195792044616853,3.2195792044616853,3.2195792044616858,3.2195792044616858,3.2195792044616853,3.2195792044616853,3.2195792044616853]
["Horn FWHM","[°]",null,10.38740589238607]
["Horn solid angle","[sr]",null,0.037236339817425364]
["filling factor",null,null,0.8]
["aperture efficiency",null,null,0.745]
["Total throughput","[m^2 sr]",{"$nulls":4},0.00025,0.00036734693877551024,0.0005625,0.0007222222222222224,0.0009,0.001224952741020794,0.0015976331360946742,0.0013912009512485138,0.00123046875,0.0010285714285714284,0.0008284023668639056,0.000418388429752066,0.0001730103806228374,0.0001189313415685148,5.839100346020762e-05,3.846153846153847e-05,1.9999999999999998e-05,1.1649408284023667e-05,6.2499999999999995e-06,3.6734693877551016e-06,2.8125e-06,1.994459833795014e-06,1.4876033057851241e-06,1.152e-06]
["focal plane area ","[m^2]",{"$nulls":4},0.006713871482153795,0.009865280545205577,0.015106210834846038,0.01939562872622208,0.02416993733575366,0.03289670109970253,0.04290521420547986,0.03736137757013051,0.03304483620122571,0.02762278552657561,0.022247148106545125,0.01123602458790201,0.004646277842320966,0.0031939589699645746,0.0015681187717833261,0.001032903304946738,0.0005371097185723036,0.00031285052024829067,0.00016784678705384487,9.865280545205575e-05,7.55310541742302e-05,5.3562188001670174e-05,3.9950309645873824e-05,3.093751978976469e-05]
["focal plane area (including efficiency effects)","[m^2]",{"$nulls":4},0.011264885037170796,0.016552484136250968,0.025345991333634292,0.03254300121849343,0.040553586133814865,0.05519580721426599,0.07198861443872459,0.06268687511766864,0.05544435604232501,0.0463469555815027,0.037327429708968324,0.018852390248157734,0.007795768191813701,0.005358991560343245,0.0026310717647371243,0.0017330592364878153,0.0009011908029736636,0.0005249169802823668,0.0002816221259292699,0.00016552484136250965,0.00012672995666817148,8.986944295582243e-05,6.703072088233863e-05,5.190859025128303e-05]
["Equivalent diameter","[m]",{"$nulls":4},0.13513675950301637,0.16381048976941456,0.20270513925452457,0.2296883245698586,0.2564039733863614,0.29913219870936575,0.34161900705208925,0.3187854045783552,0.29980494406852126,0.2741073774340766,0.2459938002613508,0.17482089094524636,0.11241896356724529,0.09320767075929116,0.06530951605407591,0.053004997977659674,0.0382224476128634,0.029171276216489697,0.021366997782196778,0.016381048976941454,0.014333417854823775,0.012070246614588442,0.010424303894417291,0.009173387427087214]
["total FP area","[m^2]",{"$nulls":4},0.49383006042566463]
["FP diameter","[m]",null,null,0.7929463798472827]
["FOV","[°]",null,null,15.056905273267676]
[]
[]
["Far sidelobes"]
["Earth RJ temperature","[K]",null,300]
["Earth solid angle","[sr]",null,5.541769440932395e-05]
["Moon RJ temperature","[K]",null,200]
["Moon solid angle","[sr]",null,7.77063855613958e-06]
["Sun RJ temperature","[K]",null,6000]
["Sun solid angle","[sr]",null,6.665602685452734e-05]
["Sidelobe signal","[Kcmb]",null,6e-09]
[]
["dTrj/dTcmb",{"$nulls":5},0.9119823548667598,0.8824989819403023,0.8498837526192877,0.814643985711614,0.7773003285236163,0.7184745437767771,0.6577707574313655,0.5967339052433085,0.5367086814224337,0.4788060730876327,0.4063647648314133,0.32530205667309414,0.23145823228677403,0.15143591902975564,0.09053738805942152,0.04925202064140435,0.02277063014549724,0.008861778546432513,0.0028845341289748666]
["Earth rejection factor wrt main beam","dB",{"$nulls":4},-111.34646728429082,-112.82812530269736,-114.1515111044512,-115.35847826587923,-116.47741812036125,-118.0331495871785,-119.48142805798247,-120.8528595346398,-122.1683200842057,-123.44247110387326,-125.09483842016434,-127.10889215887536,-129.86938392195242,-132.9774579772085,-136.44460536132723,-140.2803582453639,-144.87380641568797,-150.22816457640738,-156.34557482290717]
["Moon rejection factor wrt main beam","dB",{"$nulls":4},-101.0536372451874,-102.53529526359394,-103.8586810653478,-105.0656482267758,-106.18458808125783,-107.74031954807509,-109.18859801887905,-110.56002949553638,-111.8754900451023,-113.14964106476984,-114.80200838106092,-116.81606211977197,-119.57655388284903,-122.68462793810511,-126.15177532222381,-129.9875282062605,-134.58097637658457,-139.93533453730396,-146.05274478380375]
["Sun rejection factor wrt main beam","dB",{"$nulls":4},-125.15867693840336,-126.6403349568099,-127.96372075856374,-129.17068791999176,-130.2896277744738,-131.84535924129105,-133.293637712095,-134.66506918875234,-135.98052973831824,-137.2546807579858,-138.90704807427687,-140.9211018129879,-143.68159357606496,-146.78966763132104,-150.25681501543977,-154.09256789947645,-158.6860160698005,-164.04037423051992,-170.15778447701967]
[]
["Integrated galactic emission (from PSM)","[uK_RJ.arcmin^2]",{"$nulls":4},9833140,8047570,7389060,7343760,7653690,8506200,9635460,10938200,12360900,13871500,15985500,18738900,22713600,27316000,32446000,37781500,43666200,49769600,55612300]
["Galactic rejection factor","dB",{"$nulls":4},-68.34021477137243,-68.95159819462665,-69.90422829743116,-71.08448828123841,-72.38295206109014,-74.39733074666161,-76.3869778484949,-78.30914339656566,-80.15564627611462,-81.93053062805946,-84.19892593054429,-86.9031583569042,-90.49906891731494,-94.4084542797199,-98.62304226185611,-103.11997547015989,-108.34208567369794,-114.26463134163755,-120.86410865389551]

{"sheet":"Feuil1","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}